Connect the first gun to port 3 (C), Second to port 4 (D)
To enter the SYSTEM MENU press START+B on the light gun. (it's necessary to simultaneously release the buttons)
The calibration TEST MODE -> I/O TEST